Federal Communications Commission September 27, 2018

445 12th Street SW

Washington, DC 20554

Att: Carmell Weathers  
Wireline Competition Bureau

Subject: Network Notification No. 123

Short Term Public Notice Under Rule 51.333a

(Less than 6 months notice)

This Notice, pursuant to CFR 47, Subsections 51.325 – 51.335 advises of the following Network change(s) and/or improvement(s) within Telephone Operating Company of Vermont LLC d/b/a Consolidated Communications Inc.(“TOCOVT”).

**Vermont Wire Centers:**

| FairPoint Central Office CLLI: | Central Office Name: | FairPoint RT CLLI : | Municipality: | Route and Pole: | Street Address (if necessary): |
| --- | --- | --- | --- | --- | --- |
| RDBOVTTU | Readsboro | RDBOVT04 | Readsboro | P39 ½ RT 1 | 911 King Hill Road |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

**Planned Implementation or Retirement Date:** **11/30/2018**

**Description of Foreseeable Impact**: These network changes will create the potential for spectral interference on the CO-based ADSL and/or a Digital Design Loop (DDL) loops that share the same binder groups as the RT ADSL within the copper distribution feeder cable past the Feeder Distribution Interface (FDI).

**Description of Change**: Consolidated Communications Inc. will install Digital Subscriber Line Access Multiplexer ('DSLAM') or Litespan to provide Digital Subscriber Line (DSL) service from a Remote Terminal (RT) that is less than 30,000 feet from the Central Office.

The following loop types will be transferred to new DLC systems:

2-Wire Analog Voice Grade Loop except those circuits identified below as Services Impacted.

The following UNE loop types plus any services not specifically identified that require copper cable for provisioning will no longer be available from Consolidated’s Central Office to customer premises in the affected area:

2-Wire ADSL - Compatible Loop (ARDU) 2-Wire HDSL - Compatible Loop

4-Wire HDSL - Compatible Loop 2-Wire IDSL - Compatible Metallic Loop (ISDN)

2-Wire SDSL - Compatible Loop (HDSL 2) 2-Wire Digital Designed Metallic Loop (DDS 2)

**Attachment:** Certificate of Service

**Contact:** Rick Cimon Barbara Galardo (Regulatory)

603-315-5806 207-535-4126